**IOT Weekly report (2)**

In this week, I mainly completed the remote control of raspberry pie by Windows system of personal PC through SSH. The following are the specific steps.

1.Install the vscode, find and add the remote-ssh

截图里有图片

描述已自动生成

2. Open the plug-in configuration Shift + CTLR + P and enter “remote- SSH:settings”. Then click “Always reveal the SSH login terminal”

手机屏幕截图

描述已自动生成

3.When the installing finished, the Remote resource manager will appear in the left border, click it. Then build a new SSH target

手机屏幕的截图

描述已自动生成

4. Input C:\user\administrator\.ssh\config to enter and set remote port information 截图里有图片

描述已自动生成

Because I use DHCP on my raspberry pie, I used my hosts instead if the IP address so that the system can help me to analysis the IP

5.Connect my raspberry pie in a new window, input the password to enter it.手机屏幕的截图

描述已自动生成

6.click the “+” to build a new page, then the setting is finished

电脑屏幕的截图

描述已自动生成